*************************** START ****************************

Chip: ESP32
Download mode: uart
Start time: 20250907-15:37
Connect baud: 115200
Com:COM12
connecting...
MAC: [16, 151, 189, 193, 170, 180]
crc_cal: 19
crc_read: 19
crc_test: 0
ESP32 MAC CRC OK
manufacturer_id: 0xc8
device_id: 0x4017
fs:0x200200

Leaving...

com closed
Total use time: 10 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

Chip: ESP32
Download mode: uart
Start time: 20250907-15:37
Connect baud: 115200
Com:COM12
*************************** START ****************************

Chip: ESP32
Download mode: uart
Start time: 20250907-15:38
Connect baud: 115200
Com:COM12
connecting...
MAC: [16, 151, 189, 193, 170, 180]
crc_cal: 19
crc_read: 19
crc_test: 0
ESP32 MAC CRC OK
manufacturer_id: 0xc8
device_id: 0x4017
fs:0x200200
address/file: 0 C:\Users\Leader\Desktop\手操器LCD\3-fluidncdial固件\0-下载工具\dl_temp\bin_tmp\downloadPanel1\target.bin

Wrote 4128768 bytes (429552 compressed) at 0x00000000 in 44.8 seconds (effective 737.9 kbit/s)...

File: C:\Users\Leader\Desktop\手操器LCD\3-fluidncdial固件\0-下载工具\dl_temp\bin_tmp\downloadPanel1\target.bin
File  md5: 3980c07a486b470fa1c7ccfd951ae4f1
Flash md5: 3980c07a486b470fa1c7ccfd951ae4f1
Hash of data verified.

Leaving...

com closed
Total use time: 60 s

Download result: PASS

*************************** END ****************************



