*************************** START ****************************

Chip: ESP32
Download mode: uart
Start time: 20250902-22:33
Connect baud: 115200
Com:COM12
connecting...
MAC: [16, 151, 189, 194, 156, 168]
crc_cal: 78
crc_read: 78
crc_test: 0
ESP32 MAC CRC OK
manufacturer_id: 0xc8
device_id: 0x4017
fs:0x200000
address/file: 0 C:\Users\Leader\Desktop\手操器LCD\3-fluidncdial固件\flash_download_tool\dl_temp\bin_tmp\downloadPanel1\unospislave.ino.merged.bin

Wrote 4194304 bytes (209060 compressed) at 0x00000000 in 27.3 seconds (effective 1227.5 kbit/s)...

File: C:\Users\Leader\Desktop\手操器LCD\3-fluidncdial固件\flash_download_tool\dl_temp\bin_tmp\downloadPanel1\unospislave.ino.merged.bin
File  md5: bb6484a478463ee86bdf2835f1a91e4d
Flash md5: bb6484a478463ee86bdf2835f1a91e4d
Hash of data verified.

Leaving...

com closed
Total use time: 42 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

Chip: ESP32
Download mode: uart
Start time: 20250902-22:45
Connect baud: 115200
Com:COM12
connecting...
MAC: [16, 151, 189, 194, 156, 168]
crc_cal: 78
crc_read: 78
crc_test: 0
ESP32 MAC CRC OK
manufacturer_id: 0xc8
device_id: 0x4017
fs:0x200200
address/file: 0 C:\Users\Leader\Desktop\手操器LCD\3-fluidncdial固件\flash_download_tool\dl_temp\bin_tmp\downloadPanel1\target.bin

Wrote 4128768 bytes (429550 compressed) at 0x00000000 in 44.3 seconds (effective 746.4 kbit/s)...

File: C:\Users\Leader\Desktop\手操器LCD\3-fluidncdial固件\flash_download_tool\dl_temp\bin_tmp\downloadPanel1\target.bin
File  md5: 514201f81b7fc91e6c3ac99a24b1b75b
Flash md5: 514201f81b7fc91e6c3ac99a24b1b75b
Hash of data verified.

Leaving...

com closed
Total use time: 60 s

Download result: PASS

*************************** END ****************************



